IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2024-08-22T17:11:59"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.1.109 - Exporter 21.1.1.109 - Alternate UI 21.1.1.109"
Application: "Autodesk Revit 2021 (ENG)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENG)"

People and organizations
  Person "Lana.Whittaker" of Organization (no name given)
  Owner history of Person "Lana.Whittaker" of Organization (no name given) | application "Autodesk Revit 2021 (ENG)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENG)" | change NOCHANGE | created 1724342976 (2024-08-22T16:09:36Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "## Street City, State Zip", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 16 elements
          1 x IFCROOF | type IFCCURTAINWALLTYPE "Sloped Glazing:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Profile" | object type "Sloped Glazing:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Profile" | names: "Sloped Glazing:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Profile:2156798" | parts: 31 IFCMEMBER | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCROOF | type IFCCURTAINWALLTYPE "Sloped Glazing:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Suspension" | object type "Sloped Glazing:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Suspension" | names: "Sloped Glazing:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Suspension:2156911" | parts: 3 IFCMEMBER | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Suspension" | object type "Curtain Wall:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Suspension" | names: "Curtain Wall:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Suspension:2165843" | parts: 3 IFCMEMBER | property sets: IFC, COBie, BOS_General, NBS_Data
          12 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Cable:Cable" | object type "NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Cable:Cable" | names: "NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Cable:Cable:2166991", "NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Cable:Cable:2167585", "NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Cable:Cable:2167622" (+9 more) | material: "NBS_Concept" | property sets: COBie
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Profile" | object type "Curtain Wall:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Profile" | names: "Curtain Wall:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Profile:2171725" | parts: 31 IFCMEMBER | property sets: NBS_Data, IFC, COBie, BOS_General

Types
  IFCCURTAINWALLTYPE "Sloped Glazing:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Profile" | 1 occurrence | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCURTAINWALLTYPE "Sloped Glazing:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Suspension" | 1 occurrence | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCURTAINWALLTYPE "Curtain Wall:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Suspension" | 1 occurrence | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCBUILDINGELEMENTPROXYTYPE "NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Cable:Cable" | 12 occurrences | material: "NBS_Concept" | property sets: COBie
  IFCCURTAINWALLTYPE "Curtain Wall:NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Profile" | 1 occurrence | property sets: IFC, COBie, BOS_General, NBS_Data

Property sets
  COBie | properties | on 68 objects (68 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCTEXT)
    Material = "NBS_Soundtect_PolyesterFibrePET_White" (IFCTEXT)
  COBie | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Pr_35_93_13_80:Sound attenuator infill units" (IFCTEXT)
  COBie | properties | on 3 objects (1 IFCBUILDING, 1 IFCPROJECT, 1 IFCSITE)
    Category = "Project Information" (IFCTEXT)
  COBie | properties | on 2 objects (1 IFCCURTAINWALL, 1 IFCROOF)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_35_93_13_80:Sound attenuator infill units" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Acoustic baffle suspended ceiling system for specific areas or wall to wall acoustic ceiling installations." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Textured" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "enquiries@soundtect.com" (IFCTEXT)
    Material = "Polyester fibre (PET)" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Acoura" (IFCTEXT)
    Name = "SoundAttenuatorInfillUnits_Acoura_Profile_Soundtect" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Other,Oval,Rectangle,Crescent" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "Ten year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 2 objects (1 IFCCURTAINWALL, 1 IFCROOF)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_35_93_13_80:Sound attenuator infill units" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Acoustic baffle suspended ceiling system for specific areas or wall to wall acoustic ceiling installations." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Textured" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "enquiries@soundtect.com" (IFCTEXT)
    Material = "Polyester fibre (PET)" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Acoura" (IFCTEXT)
    Name = "SoundAttenuatorInfillUnits_Acoura_Suspension_Soundtect" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Other,Oval,Rectangle,Crescent" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "Ten year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCTEXT)
    Name = "Level 1" (IFCTEXT)
  COBie | properties | on 2 type objects
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_35_93_13_80:Sound attenuator infill units" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Acoustic baffle suspended ceiling system for specific areas or wall to wall acoustic ceiling installations." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Textured" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "enquiries@soundtect.com" (IFCTEXT)
    Material = "Polyester fibre (PET)" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Acoura" (IFCTEXT)
    Name = "SoundAttenuatorInfillUnits_Acoura_Profile_Soundtect" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Other,Oval,Rectangle,Crescent" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "Ten year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 2 type objects
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_35_93_13_80:Sound attenuator infill units" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Acoustic baffle suspended ceiling system for specific areas or wall to wall acoustic ceiling installations." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Textured" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "enquiries@soundtect.com" (IFCTEXT)
    Material = "Polyester fibre (PET)" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Acoura" (IFCTEXT)
    Name = "SoundAttenuatorInfillUnits_Acoura_Suspension_Soundtect" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Other,Oval,Rectangle,Crescent" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "Ten year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 3 objects (1 IFCBUILDING, 1 IFCPROJECT, 1 IFCSITE)
    Author (no value)
  BOS_General | properties | on 2 objects (1 IFCCURTAINWALL, 1 IFCROOF) | on 2 type objects
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Profile" (IFCTEXT)
    ManufacturerName = "Soundtect" (IFCTEXT)
    ManufacturerURL = "https://www.soundtect.com/" (IFCTEXT)
    NBSInstanceId = "ebf45587-1110-4720-8dcc-78748e762325" (IFCTEXT)
    NBSObjectId = "4a0bbc0b-d7e8-491e-9191-e0dd2766927c" (IFCTEXT)
    NBSVariantId = "00000000-0000-0000-0000-000000000000" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/4a0bbc0b-d7e8-491e-9191-e0dd2766927c/ebf45587-1110-4720-8dcc-78748e762325" (IFCTEXT)
    Uniclass2015Code = "Pr_35_93_13_80" (IFCTEXT)
    Uniclass2015Title = "Sound attenuator infill units" (IFCTEXT)
    Uniclass2015Version = "Products v1.35" (IFCTEXT)
    Version = "14" (IFCTEXT)
  BOS_General | properties | on 2 objects (1 IFCCURTAINWALL, 1 IFCROOF) | on 2 type objects
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Suspension" (IFCTEXT)
    ManufacturerName = "Soundtect" (IFCTEXT)
    ManufacturerURL = "https://www.soundtect.com/" (IFCTEXT)
    NBSInstanceId = "ebf45587-1110-4720-8dcc-78748e762325" (IFCTEXT)
    NBSObjectId = "4a0bbc0b-d7e8-491e-9191-e0dd2766927c" (IFCTEXT)
    NBSVariantId = "00000000-0000-0000-0000-000000000000" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/4a0bbc0b-d7e8-491e-9191-e0dd2766927c/ebf45587-1110-4720-8dcc-78748e762325" (IFCTEXT)
    Uniclass2015Code = "Pr_35_93_13_80" (IFCTEXT)
    Uniclass2015Title = "Sound attenuator infill units" (IFCTEXT)
    Uniclass2015Version = "Products v1.35" (IFCTEXT)
    Version = "14" (IFCTEXT)
  IFC | properties | on 4 objects (2 IFCCURTAINWALL, 2 IFCROOF) | on 4 type objects
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "USERDEFINED" (IFCTEXT)
  NBS_Data | properties | on 62 objects (62 IFCMEMBER)
    Material = "NBS_Soundtect_PolyesterFibrePET_White" (IFCTEXT)
    Profile = "NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Profile: Profile" (IFCTEXT)
  NBS_Data | properties | on 6 objects (6 IFCMEMBER)
    Material = "NBS_Soundtect_PolyesterFibrePET_White" (IFCTEXT)
    Profile = "NBS_Soundtect_SoundAttenuatorInfillUnits_Acoura_Suspension: Suspension" (IFCTEXT)
  NBS_Data | properties | on 4 objects (2 IFCCURTAINWALL, 2 IFCROOF) | on 4 type objects
    Application = "Ceiling mounting" (IFCTEXT)
    Colour = "Ballet,Bolero,Calypso,Chacha,Conga,Contemporary,Disco,Flamenco,Hiphop,Jive,Lambada,Latin,Mambo,Passo,Polka,Quickstep,Rumba,Salsa,Tango,Twist,Vogue,Waltz,Zumba" (IFCTEXT)
    ColourFastness = "Colourfastness to Light, AATCC16(3), Class 4.5" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "China" (IFCTEXT)
    CountryOfProductManufacture = "Hong Kong" (IFCTEXT)
    FirePerformanceReactionToFire = "To EN 13501, Bs1,d0" (IFCTEXT)
    Form = "Baffle" (IFCTEXT)
    Material = "Polyester fibre (PET)" (IFCTEXT)
    MoistureContentValue = "Polyester fibre when exposed to an atmosphere of 50°C at 90% relative humidity for four days showed moisture absorption of less than 0.03% by weight. Polyester is not affected by moisture" (IFCTEXT)
    Profile = "Linear" (IFCTEXT)
    Recyclability = "100%" (IFCTEXT)
    RecycledContent = "70" (IFCTEXT)
    SurfacePattern = "Solid" (IFCTEXT)