IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2024-08-12T15:13:25"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.1.109 - Exporter 21.1.1.109 - Alternate UI 21.1.1.109"
Application: "Autodesk Revit 2021 (ENG)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENG)"

People and organizations
  Person "Lana.Whittaker" of Organization (no name given)
  Owner history of Person "Lana.Whittaker" of Organization (no name given) | application "Autodesk Revit 2021 (ENG)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENG)" | change NOCHANGE | created 1723471135 (2024-08-12T13:58:55Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | object type "Level:Circle Head - Project Datum" | elevation 0.
        contains 2 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony" | object type "Basic Wall:NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony" | names: "Basic Wall:NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony:221796" | material: layers "Basic Wall:NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony" ("NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony" 25.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony" | object type "Compound Ceiling:NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony" | CEILING | names: "Compound Ceiling:NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony:221960" | material: layers "Compound Ceiling:NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony" ("NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony" 25.) | property sets: IFC, COBie, BOS_General, NBS_Data

Types
  IFCWALLTYPE "Basic Wall:NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony" | STANDARD | 1 occurrence | material: layers "Basic Wall:NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony" ("NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony" 25.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Compound Ceiling:NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony" | CEILING | 1 occurrence | property sets: IFC, COBie, BOS_General, NBS_Data

Property sets
  COBie | properties | on 3 objects (1 IFCBUILDING, 1 IFCPROJECT, 1 IFCSITE)
    Category = "Project Information" (IFCTEXT)
  COBie | properties | on 2 objects (1 IFCCOVERING, 1 IFCWALLSTANDARDCASE)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_35_93_13_80:Sound attenuator infill units" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Slatted acoustic wall and ceiling covering" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "enquiries@soundtect.com" (IFCTEXT)
    Material = "Polyester fibre (PET)" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Harmony" (IFCTEXT)
    Name = "SoundAttenuatorInfillUnits_Harmony_Soundtect" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle,Square" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "Ten year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCTEXT)
    Name = "Level 0" (IFCTEXT)
  COBie | properties | on 2 type objects
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_35_93_13_80:Sound attenuator infill units" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Slatted acoustic wall and ceiling covering" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "enquiries@soundtect.com" (IFCTEXT)
    Material = "Polyester fibre (PET)" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Harmony" (IFCTEXT)
    Name = "SoundAttenuatorInfillUnits_Harmony_Soundtect" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangle,Square" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "Ten year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 3 objects (1 IFCBUILDING, 1 IFCPROJECT, 1 IFCSITE)
    Author (no value)
  BOS_General | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony" (IFCTEXT)
    ManufacturerName = "Soundtect" (IFCTEXT)
    ManufacturerURL = "https://www.soundtect.com/" (IFCTEXT)
    NBSInstanceId = "05605919-286a-477c-a38c-5bf7334f6d27" (IFCTEXT)
    NBSObjectId = "28b3ac30-025e-44d5-8e35-855c6d9d9bec" (IFCTEXT)
    NBSVariantId = "00000000-0000-0000-0000-000000000000" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/28b3ac30-025e-44d5-8e35-855c6d9d9bec/05605919-286a-477c-a38c-5bf7334f6d27" (IFCTEXT)
    Uniclass2015Code = "Pr_35_93_13_80" (IFCTEXT)
    Uniclass2015Title = "Sound attenuator infill units" (IFCTEXT)
    Uniclass2015Version = "Products v1.35" (IFCTEXT)
    Version = "9" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_Soundtect_SoundAttenuatorInfillUnits_Harmony" (IFCTEXT)
    ManufacturerName = "Soundtect" (IFCTEXT)
    ManufacturerURL = "https://www.soundtect.com/" (IFCTEXT)
    NBSInstanceId = "a046b862-755c-488e-875d-e3f40b61fb04" (IFCTEXT)
    NBSObjectId = "28b3ac30-025e-44d5-8e35-855c6d9d9bec" (IFCTEXT)
    NBSVariantId = "00000000-0000-0000-0000-000000000000" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/28b3ac30-025e-44d5-8e35-855c6d9d9bec/a046b862-755c-488e-875d-e3f40b61fb04" (IFCTEXT)
    Uniclass2015Code = "Pr_35_93_13_80" (IFCTEXT)
    Uniclass2015Title = "Sound attenuator infill units" (IFCTEXT)
    Uniclass2015Version = "Products v1.35" (IFCTEXT)
    Version = "10" (IFCTEXT)
  IFC | properties | on 2 objects (1 IFCCOVERING, 1 IFCWALLSTANDARDCASE) | on 2 type objects
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "USERDEFINED" (IFCTEXT)
  NBS_Data | properties | on 2 objects (1 IFCCOVERING, 1 IFCWALLSTANDARDCASE) | on 2 type objects
    AcousticPerformanceSoundAbsorption = "NRC 0.75 (20 mm)" (IFCTEXT)
    Application = "Ceiling mounting,Wall mounting" (IFCTEXT)
    Colour = "Ballet,Bolero,Calypso,Chacha,Conga,Contemporary,Disco,Flamenco,Hiphop,Jive,Lambada,Latin,Mambo,Passo,Polka,Quickstep,Rumba,Salsa,Tango,Twist,Vogue,Waltz,Zumba,Ebony,White oak,Pine,Oak,Walnut,Chestnut" (IFCTEXT)
    ColourFastness = "Colourfastness to Light, AATCC16(3), Class 4.5" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "China" (IFCTEXT)
    CountryOfProductManufacture = "Hong Kong" (IFCTEXT)
    DimensionsSizeLengthxWidth = "2400 x 600 mm" (IFCTEXT)
    DimensionsThicknessOverall = "25 mm" (IFCTEXT)
    FirePerformanceReactionToFire = "To EN 13501, Bs1,d0" (IFCTEXT)
    Form = "Panel,Raft" (IFCTEXT)
    Material = "Polyester fibre (PET)" (IFCTEXT)
    MaterialDensity = "10 mm, 2 kg/m²,20 mm, 4 kg/m²" (IFCTEXT)
    MoistureContentValue = "Polyester fibre when exposed to an atmosphere of 50°C at 90% relative humidity for four days showed moisture absorption of less than 0.03% by weight. Polyester is not affected by moisture" (IFCTEXT)
    Profile = "Linear" (IFCTEXT)
    Recyclability = "100%" (IFCTEXT)
    RecycledContent = "70" (IFCTEXT)
    SurfacePattern = "Solid" (IFCTEXT)